BLOCKS
	MAIN

	RAIL A=RED WIRE
RAIL B=BLACK WIRE
EAST=BLACK / ORANGE 
WEST:  BLACK / RED
PM42 ZONE (1) = MAIN (M)

	BLOCK
	TAPE COLOR
	
	

	M1
	BLK
	
	

	M2
	GRY
	
	

	M3
	ORG
	
	

	M4
	BLK / RED
	
	

	M5
	GRN
	
	

	M6
	RED
	
	

	M7
	YEL
	
	

	M8
	PUR
	
	

	M9
	BLU
	
	

	M10
	WHT
	
	

	M11
	BRN
	
	

	M12
	WHT / BLU
	
	



	BRANCH

	RAIL A=WHITE WIRE
RAIL B=BLACK WIRE
EAST=BLACK / WHITE
WEST=BLACK / BROWN
PM42 ZONE (2) = BRANCH (B)

	BLOCK
	TAPE COLOR
	
	

	B1
	BLU
	
	

	B2
	RED
	
	

	B3
	GRY
	
	

	B4
	BLK
	
	

	B5
	GRN
	
	

	B6
	PUR
	
	

	B7
	YEL
	
	

	B8
	WHT
	
	





	CENTRAL AREA

	RAIL A=RED WIRE (FROM MAIN POWER=RED/ORANGE/YELLOW)
RAIL B=BLACK WIRE
EAST=BLACK / PURPLE
WEST=BLACK / GREEN
C10 + C 11=BLACK / GRAY/RED
C EXTENSION FROM MAIN POWER=BLACK/BLUE
PM42 ZONE (3) = CENTRAL (C)

	BLOCK
	TAPE COLOR
	
	

	C1
	ORG
	
	

	C2
	RED
	
	

	C3
	WHT
	
	

	C4
	YEL
	
	

	C5
	BLK
	
	

	C6
	PUR
	
	

	C7
	GRN
	
	

	C8
	BRN
	
	

	C9
	GRY
	
	

	C10
	BLU
	
	

	C11
	WHT / BLU
	
	





	YARD

	RAIL A=WHITE WIRE
RAIL B=BLACK WIRE
FROM POWER TO MAIN YARD=BLACK / YELLOW
FROM POWER TO REVERSING SECTION=BLACK /RED
PM42 ZONE (4) = YARD (Y)

	BLOCK
	TAPE COLOR
	
	

	Y1
	YEL/BLK
	
	

	Y2
	YEL/BLK
	
	


NO BLOCKS FOR YARD.
WHITE WIRE WITH YELLOW / BLACK TAPE IS SINGLE RUN FROM POWER TO ALL OF YARD.
NEED TO T THE WHITE WIRE WITH YELLOW / BLACK TAPE TO FEE THE REVERSING SECTION.
WHITE WIRE WITH RED / BLACK TAPE NO USED.  WAS INTENDED FOR REVERSING LOOP (Y2), BUT NOT USED.


TURNOUTS
	MAIN
	
	
	
	
	

	TURNOUT NO.
	TYPE
	WIRE COLOR
	TAPE COLOR
	
	

	SM01
	No. 8 Left Straight
	
	
	
	

	SM02
	No. 8 Right Curved
	
	
	
	

	SM03
	No. 6 Left Straight
	
	
	
	

	SM04
	No. 5 Right Straight
	
	
	
	

	SM05
	No. 8 Left Curved
	
	
	
	

	SM06
	No. 8 Right Curved
	
	
	
	

	SM07
	No. 5 Left Straight
	
	
	
	



	BRANCH
	
	
	

	TURNOUT NO.
	TYPE
	WIRE COLOR
	TAPE COLOR

	SB01
	No. 5 Right Straight
	
	

	SB02
	No. 6 Left Straight
	
	

	SB03
	No. 6 Right Straight
	
	

	SB04
	No. 7 Right Curved
	
	

	SB05
	No. 6 Right Straight
	
	

	SB06
	No. 6 Three Way (N—PAIRED)
	
	

	SB07
	No. 6 Three Way (S—PAIRED)
	
	

	SB08
	No. 7.5 Left Curved
	
	

	SB09
	No. 6 Right Straight
	
	

	SB10
	No. 8 Right Curved
	
	

	
	
	
	



	CENTRAL
	
	
	

	TURNOUT NO.
	TYPE
	WIRE COLOR
	TAPE COLOR

	SC01
	No.  Right Curved
	
	

	
	
	
	



	YARD
	
	
	

	TURNOUT NO.
	TYPE
	WIRE COLOR
	TAPE COLOR

	Y01
	
	
	

	Y02
	
	
	

	Y03
	
	
	

	Y04
	
	
	

	Y05
	
	
	





	SE8C No. 1

	TURNOUT NO.
	PANEL PUSHBUTTON
(BOARD TO PANEL)
	SWITCH MACHINE (AND LED)
(BOARD TO PANEL TO SWITCH MACHINE)

	
	TERMINAL STRIP (VE+)
(TAPE / WHITE WIRE)
	PIN NO.
(TAPE / COLORED WIRE)
	PIN NO.
(TAPE / WHITE WIRE)
(TO TORTOISE PIN 1)
	PIN NO.
(TAPE / COLORED WIRE)
(TO TORTOISE PIN 8)

	SM01
	P2—YEL / WHT
	P4—YEL / ORG
	PD—RED / WHT
	PE—RED / ORG

	SMO2
	P2—YEL / WHT
	P6—YEL / BLU
	PF—RED / WHT
	PH—RED / GRN

	SMO3
	P2—YEL / WHT
	P8—YEL / BRN
	PJ—RED / WHT
	PK—RED / BLU

	SM04
	P2—YEL / WHT
	P10—YEL / GRN
	PL—RED / WHT
	PM—RED / BRN

	SM05
	P2—ORG / WHT
	P12—ORG / ORG
	PN—BRN / WHT
	PP—BRN / BRN

	SM06
	P2—ORG / WHT
	P14—ORG / BLU
	PR—BRN / WHT
	PS—BRN / BLU

	SM07
	P2—ORG / WHT
	P16—ORG / BRN
	PT—BRN / WHT
	PU—BRN / ORG

	UNASSIGNED[footnoteRef:1] [1:  Terminates at SM08] 

	P2—ORG / WHT
	P18—ORG / GRN
	PV—BRN / WHT
	PW—BRN / GRN



	SE8C No. 2

	TURNOUT NO.
	PANEL PUSHBUTTON
(BOARD TO PANEL)
	SWITCH MACHINE (AND LED)
(BOARD TO PANEL TO SWITCH MACHINE)

	
	TERMINAL STRIP (VE+)
(TAPE / WHITE WIRE)
	PIN NO.
(TAPE / COLORED WIRE)
	PIN NO.
(TAPE / WHITE WIRE)
	PIN NO.
(TAPE / COLORED WIRE)

	SB01
	P2—GRN / WHT
	P4—GRN / ORG
	PD—WHT / WHT
	PE—WHT / ORG

	SBO2
	P2—GRN / WHT
	P6—GRN / BLU
	PF—WHT / WHT
	PH—WHT / BLU

	SBO3
	P2—GRN  / WHT
	P8—GRN / BRN
	PJ—WHT / WHT
	PK—WHT / BRN

	SB04
	P2—GRN  / WHT
	P10—GRN / GRN
	PL—WHT / WHT
	PM—WHT / GRN

	SB05
	P2—BLK / WHT
	P12—BLK / ORG
	PN—PUR / WHT
	PP—PUR / ORG

	SB06
	P2—BLK / WHT
	P14—BLK / BLU
	PR—PUR / WHT
	PD—PUR / BLU

	SB07
	P2—BLK / WHT
	P16—BLK / BRN
	PT—PUR / WHT
	PU—PUR / BRN

	SB08
	P2—BLK / WHT
	P18—BLK / GRN
	PV—PUR / WHT
	PW—PUR / GRN





	SE8C No. 3

	TURNOUT NO.
	PANEL PUSHBUTTON
(BOARD TO PANEL)
	SWITCH MACHINE (AND LED)
(BOARD TO PANEL TO SWITCH MACHINE)

	
	TERMINAL STRIP (VE+)
(TAPE / WHITE WIRE)
	PIN NO.
(TAPE / COLORED WIRE)
	PIN NO.
(TAPE / WHITE WIRE)
	PIN NO.
(TAPE / COLORED WIRE)

	SB09
	P2—GRY / WHT
	P4—GRY / ORG
	PD—BLU / WHT
	PE—BLU / ORG

	SB10
	P2—GRY / WHT
	P6—GRY / BLU
	PF—BLU / WHT 
	PH—BLU / BLU

	SC01
	P2—GRY / WHT
	P8—GRY / BRN
	PJ—BLU / WHT
	PK—BLU / BRN

	UNASSIGNED
	P2—GRY / WHT
	P10—GRY / GRN
	PL—BLU / GRN
	PM—BLU / GRN[footnoteRef:2] [2:  Terminates at control panel.] 


	UNASSIGNED
	P2—
	P12—
	PN—
	PP—

	UNASSIGNED
	P2—
	P14—
	PR—
	PD—

	UNASSIGNED
	P2—
	P16—
	PT—
	PU—

	UNASSIGNED
	P2—
	P18—
	PV—
	PW—



	SE8C No. [____] 

	TURNOUT NO.
	PANEL PUSHBUTTON
(BOARD TO PANEL)
	SWITCH MACHINE (AND LED)
(BOARD TO PANEL TO SWITCH MACHINE)

	
	TERMINAL STRIP (VE+)
(TAPE / WHITE WIRE)
	PIN NO.
(TAPE / COLORED WIRE)
	PIN NO.
(TAPE / WHITE WIRE)
	PIN NO.
(TAPE / COLORED WIRE)

	UNASSIGNED
	P2—
	P4—
	PD—
	PE—

	UNASSIGNED
	P2—
	P6—
	PF— 
	PH—

	UNASSIGNED
	P2—
	P8—
	PJ—
	PK—

	UNASSIGNED
	P2—
	P10—
	PL—
	PM—

	UNASSIGNED
	P2—
	P12—
	PN—
	PP—

	UNASSIGNED
	P2—
	P14—
	PR—
	PD—

	UNASSIGNED
	P2—
	P16—
	PT—
	PU—

	UNASSIGNED
	P2—
	P18—
	PV—
	PW—
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