BLOCKS
	MAIN

	RAIL A=RED WIRE
RAIL B=BLACK WIRE
EAST=BLACK / ORANGE 
WEST:  BLACK / RED
PM42 ZONE (1) = MAIN (M)

	BLOCK
	TAPE COLOR
	
	

	M1
	BLK
	
	

	M2
	GRY
	
	

	M3
	ORG
	
	

	M4
	BLK / RED
	
	

	M5
	GRN
	
	

	M6
	RED
	
	

	M7
	YEL
	
	

	M8
	PUR
	
	

	M9
	BLU
	
	

	M10
	WHT
	
	

	M11
	BRN
	
	

	M12
	WHT / BLU
	
	



	BRANCH

	RAIL A=WHITE WIRE
RAIL B=BLACK WIRE
EAST=BLACK / WHITE
WEST=BLACK / BROWN
PM42 ZONE (2) = BRANCH (B)

	BLOCK
	TAPE COLOR
	
	

	B1
	BLU
	
	

	B2
	RED
	
	

	B3
	GRY
	
	

	B4
	BLK
	
	

	B5
	GRN
	
	

	B6
	PUR
	
	

	B7
	YEL
	
	

	B8
	WHT
	
	





	CENTRAL AREA

	RAIL A=RED WIRE (FROM MAIN POWER=RED/ORANGE/YELLOW)
RAIL B=BLACK WIRE
EAST=BLACK / PURPLE
WEST=BLACK / GREEN
C10 + C 11=BLACK / GRAY/RED
C EXTENSION FROM MAIN POWER=BLACK/BLUE
PM42 ZONE (3) = CENTRAL (C)

	BLOCK
	TAPE COLOR
	
	

	C1
	ORG
	
	

	C2
	RED
	
	

	C3
	WHT
	
	

	C4
	YEL
	
	

	C5
	BLK
	
	

	C6
	PUR
	
	

	C7
	GRN
	
	

	C8
	BRN
	
	

	C9
	GRY
	
	

	C10
	BLU
	
	

	C11
	WHT / BLU
	
	





	YARD

	RAIL A=WHITE WIRE
RAIL B=BLACK WIRE
FROM POWER TO MAIN YARD=BLACK / YELLOW
FROM POWER TO REVERSING SECTION=BLACK /RED
PM42 ZONE (4) = YARD (Y)

	BLOCK
	TAPE COLOR
	
	

	Y1
	YEL / BLK
	
	

	Y2
	YEL / BLK
	
	


NO BLOCKS FOR YARD.
WHITE WIRE WITH YELLOW / BLACK TAPE IS SINGLE RUN FROM POWER TO ALL OF YARD.
NEED TO T THE WHITE WIRE WITH YELLOW / BLACK TAPE TO FEE THE REVERSING SECTION.
WHITE WIRE WITH RED / BLACK TAPE NO USED.  WAS INTENDED FOR REVERSING LOOP (Y2), BUT NOT USED.

TURNOUTS
	MAIN
	
	
	
	
	

	TURNOUT NO.
	TYPE
	WIRE COLOR
	TAPE COLOR
	
	

	SM01
	No. 8 Left Straight
	
	
	
	

	SM02
	No. 8 Right Curved
	
	
	
	

	SM03
	No. 6 Left Straight
	
	
	
	

	SM04
	No. 5 Right Straight
	
	
	
	

	SM05
	No. 8 Left Curved
	
	
	
	

	SM06
	No. 8 Right Curved
	
	
	
	

	SM07
	No. 5 Left Straight
	
	
	
	



	BRANCH
	
	
	

	TURNOUT NO.
	TYPE
	WIRE COLOR
	TAPE COLOR

	SB01
	No. 5 Right Straight
	
	

	SB02
	No. 6 Left Straight
	
	

	SB03
	No. 6 Right Straight
	
	

	SB04
	No. 7 Right Curved
	
	

	SB05
	No. 6 Right Straight
	
	

	SB06
	No. 6 Three Way (N—PAIRED)
	
	

	SB07
	No. 6 Three Way (S—PAIRED)
	
	

	SB08
	No. 7.5 Left Curved
	
	

	SB09
	No. 6 Right Straight
	
	

	SB10
	No. 8 Right Curved
	
	

	
	
	
	



	CENTRAL
	
	
	

	TURNOUT NO.
	TYPE
	WIRE COLOR
	TAPE COLOR

	SC01
	No.  Right Curved
	
	

	
	
	
	



	SE8C No. 1

	TURNOUT NO.
	PANEL PUSHBUTTON
(BOARD TO PANEL)
	SWITCH MACHINE (AND LED)
(BOARD TO PANEL TO SWITCH MACHINE)

	
	TERMINAL STRIP (VE+)
(TAPE / WHITE WIRE)
	PIN NO.
(TAPE / COLORED WIRE)
	PIN NO.
(TAPE / WHITE WIRE)
(TO TORTOISE PIN 1)
	PIN NO.
(TAPE / COLORED WIRE)
(TO TORTOISE PIN 8)

	
	PIN
	TAPE
	WIRE
	PIN
	TAPE
	WIRE
	PIN
	TAPE
	WIRE
	PIN
	TAPE
	WIRE

	SM01
	2
	YEL
	WHT
	4
	YEL 
	ORG
	D
	RED
	WHT
	E
	RED 
	ORG

	SM02
	2
	YEL
	WHT
	6
	YEL
	BLU
	F
	RED 
	WHT
	H
	RED
	GRN

	SM03
	2
	YEL
	WHT
	8
	YEL
	BRN
	J
	RED
	WHT
	K
	RED
	BLU

	SM04
	2
	YEL
	WHT
	10
	YEL
	GRN
	L
	RED 
	WHT
	M
	RED
	BRN

	SM05
	2
	ORG
	WHT
	12
	ORG 
	ORG
	N
	BRN
	WHT
	P
	BRN 
	BRN

	SM06
	2
	ORG 
	WHT
	14
	ORG 
	BLU
	R
	BRN 
	WHT
	S
	BRN 
	BLU

	SM07
	2
	ORG 
	WHT
	16
	ORG 
	BRN
	T
	BRN 
	WHT
	U
	BRN 
	ORG

	UNASSIGNED
	2
	ORG 
	WHT
	18
	ORG 
	GRN
	V
	BRN 
	WHT
	W
	BRN 
	GRN[footnoteRef:1] [1:  Terminates at SM08] 




	SE8C No. 2

	TURNOUT NO.
	PANEL PUSHBUTTON
(BOARD TO PANEL)
	SWITCH MACHINE (AND LED)
(BOARD TO PANEL TO SWITCH MACHINE)

	
	TERMINAL STRIP (VE+)
(TAPE / WHITE WIRE)
	PIN NO.
(TAPE / COLORED WIRE)
	PIN NO.
(TAPE / WHITE WIRE)
	PIN NO.
(TAPE / COLORED WIRE)

	
	PIN
	TAPE
	WIRE
	PIN
	TAPE
	WIRE
	PIN
	TAPE
	WIRE
	PIN
	TAPE
	WIRE

	SB01
	2
	GRN
	WHT
	4
	GRN 
	ORG
	D
	WHT
	WHT
	E
	WHT 
	ORG

	SB02
	2
	GRN
	WHT
	6
	GRN
	BLU
	F
	WHT 
	WHT
	H
	WHT 
	BLU

	SB03
	2
	GRN
	WHT
	8
	GRN
	BRN
	J
	WHT 
	WHT
	K
	WHT 
	BRN

	SB04
	2
	GRN
	WHT
	10
	GRN
	GRN
	L
	WHT 
	WHT
	M
	WHT 
	GRN

	SB05
	2
	BLK
	WHT
	12
	BLK 
	ORG
	N
	PUR
	WHT
	P
	PUR 
	ORG

	SB06
	2
	BLK
	WHT
	14
	BLK 
	BLU
	R
	PUR 
	WHT
	S
	PUR 
	BLU

	SB07
	2
	BLK
	WHT
	16
	BLK 
	BRN
	T
	PUR 
	WHT
	U
	PUR 
	BRN

	SB08
	2
	BLK
	WHT
	18
	BLK 
	GRN
	V
	PUR 
	WHT
	W
	PUR 
	GRN





	SE8C No. 3

	TURNOUT NO.
	PANEL PUSHBUTTON
(BOARD TO PANEL)
	SWITCH MACHINE (AND LED)
(BOARD TO PANEL TO SWITCH MACHINE)

	
	TERMINAL STRIP (VE+)
(TAPE / WHITE WIRE)
	PIN NO.
(TAPE / COLORED WIRE)
	PIN NO.
(TAPE / WHITE WIRE)
	PIN NO.
(TAPE / COLORED WIRE)

	
	PIN
	TAPE
	WIRE
	PIN
	TAPE
	WIRE
	PIN
	TAPE
	WIRE
	PIN
	TAPE
	WIRE

	SB09
	2
	GRY
	WHT
	4
	GRY
	ORG
	D
	BLU
	WHT
	E
	BLU
	ORG

	SB10
	2
	GRY
	WHT
	6
	GRY
	BLU
	F
	BLU
	WHT
	H
	BLU
	BLU

	SC01
	2
	GRY
	WHT
	8
	GRY
	BRN
	J
	BLU
	WHT
	K
	BLU
	BRN

	UNASSIGNED
	2
	GRY
	WHT
	10
	GRY
	GRN
	L
	BLU
	WHT
	M
	BLU
	GRN[footnoteRef:2] [2:  Terminates at control panel.] 


	UNASSIGNED
	2
	?
	WHT
	12
	?
	ORG
	N
	?
	WHT
	P
	?
	ORG

	UNASSIGNED
	2
	?
	WHT
	14
	?
	BLU
	R
	?
	WHT
	D
	?
	BLU

	UNASSIGNED
	2
	?
	WHT
	16
	?
	BRN
	T
	?
	WHT
	U
	?
	BRN

	UNASSIGNED
	2
	?
	WHT
	18
	?
	GRN
	V
	?
	WHT
	W
	?
	GRN
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